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    IQCS

First written test
ESD compliance verifier
	Field
	Quality area
	Qualification
	ESD compliance verifier
	Valid date
	2020

	Exam type
	Multiple choice
	No. of Ques.
	40
	Exam hour
	90 minutes

	Title
	Sub title
	Detail
	No. of Ques.
	Distribution

	ANSI/ESD
S20.20 
	1. ESD Control program
	· ESD control program requirements
· ESD control program manager of coordinator
	10
	25%

	
	2. ESD control program
Administration requirements
	· ESD control program plan
· Training plan
· Product qualification plan
· Compliance verification plan
	
	

	
	3. ESD control program
technical requirements
	· Grounding/Equipotential
· Personnel grounding 
· Package and marking
	
	

	ESD TR-53
테스트 장비
	1. Test equipment(1)
	· AC outlet analytzer
· AC circuit tester 
· Charged plate monitor(CPM)
· DC Ohmmeter
	10
	25%

	
	2. Test equipment (2)
	· Concentric ring electrode assembly
· Electrostatic field meter
· Electrostatic voltage meter
· Foot electrode
· Hand-held electrode
· Insulative support surface 
· Integrated checker
· Resistance measurement apparatus
· Resistance measurement electrodes 
· Two-point probe
	
	

	Compliance verification of ESD protective equipment and materials
	1. ESD protective equipment and materials
	· Grounding/Bonding systems
· Worksurfaces 
· Wrist straps
· Constant monitors
· Footwear
· Flooring 
· Garments 
· Ionizer  
· Seating 
· Mobile equipment(Carts)
· Elecrical soldering/Disoldering hand toos
· Gloves and finger cots
· Packaging
	20
	50%







2nd practical test
ESD compliance verifier
	Field
	Quality area
	Qualification
	ESD compliance verifier
	Valid date
	2020

	Exam type
	Short answer
	No. of Ques.
	10-20
	Exam hour
	120 minutes

	Title
	Sub title
	Detail
	No. of Ques.
	Distribution

	Compliance verification of ESD protective equipment and materials
	Compliance verification practice of ESD protection equipment 
	· Charged plate monitor(CPM)
· Concentric ring electrode assembly
· Electrostatic field meter
· Foot electrode
· Hand-held electrode
· Insulative support surface 
· Integrated checker
· Resistance measurement apparatus
· Resistance measurement electrodes 
· Two-point probe
	20
	50%

	
	Compliance verification practice of ESD materials 
	· Grounding/Bonding systems
· Worksurfaces 
· Wrist straps
· Constant monitors
· Footwear
· Flooring 
· Garments 
· Ionizer  
· Seating 
· Mobile equipment(Carts)
· Elecrical soldering/Disoldering hand toos
· Gloves and finger cots
· Packaging
	Depends on percentage
	100%
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